**Załącznik nr 1A – CENY jednostkowe**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Lp** | **Nr katalogowy** | **Opis** | **Ilość** | **Cena jednostkowa****netto** | **Cena razem****netto** |
| **1.0** | **C1-AIR-CT5520-K9** | Cisco ONE - 5520 Wireless Controller w/rack mounting kit | 1 |  |  |
| 1.0.1 | shared-suport ~~CT5520K9~~ | shared-support 8X5XNBD Cisco 5520 Wireless Controller  | 1 |  |  |
| 1.1 | CAB-9K10A-EU | Power Cord, 250VAC 10A CEE 7/7 Plug, EU | 2 |  |  |
| 1.2 | LIC-CT5520-DTLS-K9 | Cisco 5520 Wireless Controller DTLS License | 1 |  |  |
| 1.3 | AIR-CT5520-SW-8.2 | Cisco 5520 Wireless Controller SW Rel. 8.2 | 1 |  |  |
| 1.4 | AIR-PSU1-770W | 770W AC Hot-Plug Power Supply for 5520 Controller | 1 |  |  |
| 1.5 | AIR-CT6870-NIC-K9 | PCIe Network Interface 20G | 1 |  |  |
| 1.6 | AIR-BZL-C220M4 | Cisco 5520 Wireless Controller Security Bezel | 1 |  |  |
| 1.7 | AIR-PSU1-770W | 770W AC Hot-Plug Power Supply for 5520 Controller | 1 |  |  |
| 1.8 | AIR-CPU-E52609D | 1.90 GHz E5-2609 v3/85W 6C/15MB Cache/DDR4 1600MHz | 1 |  |  |
| 1.9 | AIR-SD-32G-S | 32GB SD Card for UCS servers | 1 |  |  |
| 1.10 | AIR-SD240GBKS4-EV | 240GB 2.5 inch Enterprise Value 6G SATA SSD | 1 |  |  |
| 1.11 | AIR-MR-1X081RU-A | 8GB DDR4-2133-MHz RDIMM/PC4-17000/single rank/x4/1.2v | 4 |  |  |
| 1.12 | AIR-TPM2-001 | Trusted Platform Module 1.2 for UCS (SPI-based) | 1 |  |  |
| ~~1.13~~ | ~~DNA-VOUCHER~~ | ~~Tracker Eligibility SKU for DNA Offers~~ | ~~1~~ |  |  |
| 1.14 | C1-MSE-PAK | Cisco ONE MSE License PAK | 1 |  |  |
| 1.15 | C1FPAIRK9 | Cisco ONE Foundation Perpetual - Wireless | 200 |  |  |
| 1.15.0.1 | Shared-support~~CON-ECMU-C1FPAIR~~ | SWSS UPGRADES C1 Foundation Perpetual - Wireless | 200 |  |  |
| 1.16 | C1-WLC-1 | Cisco ONE Wireless LAN Controller AP License (any WLC) | 200 |  |  |
| 1.17 | C1-WLC-PAK | Cisco ONE Wireless LAN Controller AP License PAK (any WLC) | 1 |  |  |
| 1.18 | C1-PI-LFAS-AP-K9 | Cisco ONE PI Device License for LF & AS for WLAN | 200 |  |  |
| 1.19 | C1-ISE-BASE-AP | Cisco ONE Identity Services Engine 25 EndPoint Base Lic | 200 |  |  |
| 1.20 | C1-MSE-LS-1 | Cisco ONE CMX OnPrem Base (Location + Connect) - 1AP license | 200 |  |  |
| ~~1.21~~ | ~~C1-CEM-25-K9~~ | ~~Cisco ONE Energy Mgmt Perpetual Lic - 25 DO End Points~~ | ~~200~~ |  |  |
| ~~1.22~~ | ~~C1-LC-5-1Y~~ | ~~Cisco ONE StealthWatch 5 FPS Lic 1 YR~~ | ~~200~~ |  |  |
| 1.23 | C1F1VAIR-03 | Tracker PID v03 Fnd Perpetual AIR - no delivery | 1 |  |  |
| **2.0** | **C1-AIR-CT5520-K9** | Cisco ONE - 5520 Wireless Controller w/rack mounting kit | 1 |  |  |
| 2.0.1 | shared-suport ~~CT5520K9~~ | shared-support 8X5XNBD Cisco 5520 Wireless Controller  | 1 |  |  |
| 2.1 | CAB-9K10A-EU | Power Cord, 250VAC 10A CEE 7/7 Plug, EU | 2 |  |  |
| 2.2 | LIC-CT5520-DTLS-K9 | Cisco 5520 Wireless Controller DTLS License | 1 |  |  |
| 2.3 | AIR-CT5520-SW-8.2 | Cisco 5520 Wireless Controller SW Rel. 8.2 | 1 |  |  |
| 2.4 | AIR-PSU1-770W | 770W AC Hot-Plug Power Supply for 5520 Controller | 1 |  |  |
| 2.5 | AIR-CT6870-NIC-K9 | PCIe Network Interface 20G | 1 |  |  |
| 2.6 | AIR-BZL-C220M4 | Cisco 5520 Wireless Controller Security Bezel | 1 |  |  |
| 2.7 | AIR-PSU1-770W | 770W AC Hot-Plug Power Supply for 5520 Controller | 1 |  |  |
| 2.8 | AIR-CPU-E52609D | 1.90 GHz E5-2609 v3/85W 6C/15MB Cache/DDR4 1600MHz | 1 |  |  |
| 2.9 | AIR-SD-32G-S | 32GB SD Card for UCS servers | 1 |  |  |
| 2.10 | AIR-SD240GBKS4-EV | 240GB 2.5 inch Enterprise Value 6G SATA SSD | 1 |  |  |
| 2.11 | AIR-MR-1X081RU-A | 8GB DDR4-2133-MHz RDIMM/PC4-17000/single rank/x4/1.2v | 4 |  |  |
| 2.12 | AIR-TPM2-001 | Trusted Platform Module 1.2 for UCS (SPI-based) | 1 |  |  |
| **3.0** | **SFP-H10GB-CU3M=** | 10GBASE-CU SFP+ Cable 3 Meter | 4 |  |  |
| **4.0** | **AIR-AP2802I-E-K9** | 802.11ac W2 AP w/CA; 4x4:3; Int Ant; 2xGbE E | 20 |  |  |
| 4.0.1 | shared-support ~~ARAPIEK9~~ | shared-support 8X5XNBD 802.11ac W2 AP w/CA; | 20 |  |  |
| 4.1 | AIR-AP-T-RAIL-R | Ceiling Grid Clip for Aironet APs - Recessed Mount (Default) | 20 |  |  |
| 4.2 | AIR-AP-BRACKET-1 | 802.11n AP Low Profile Mounting Bracket (Default) | 20 |  |  |
| 4.3 | SW2802-CAPWAP-K9 | Cisco Aironet 2800 Series CAPWAP Software Image | 20 |  |  |
| SUMA (pozycje 1.0 – 4.3)  |  |